Data File  : C:\Users\P...s\ChemStation\1\Data\default 2025-02-06 13-53-32\F-003-103-NUG_SS.D
Acq. Method: terps and cannabs 20 min.M


The Acq. Method's Instrument Parameters for the Run were : 


=====================================================================
                             Agilent 8890
=====================================================================

Module Type: GC
Module Name: Agilent 8890
GC
GC Summary
Run Time                                     20 min
Post Run Time                                0 min

Oven
Temperature
Setpoint                                     On
(Initial)                                    40 °C
Hold Time                                    3.2 min
Post Run                                     50 °C
Program
#1 Rate                                      25 °C/min
#1 Value                                     250 °C
#1 Hold Time                                 8.4 min


Equilibration Time                           1 min
Max Temperature                              350 °C
Maximum Temperature Override                 Disabled
Slow Fan                                     Disabled

ALS
Front Injector
Syringe Size                                 10 μL
Injection Volume                             1 μL
Solvent A Washes (PreInj)                    3
Solvent A Washes (PostInj)                   3
Solvent A Volume                             8 μL
Solvent B Washes (PreInj)                    3
Solvent B Washes (PostInj)                   3
Solvent B Volume                             8 μL
Sample Washes                                2
Sample Wash Volume                           1 μL
Sample Pumps                                 6
Dwell Time (PreInj)                          0 min
Dwell Time (PostInj)                         0 min
Solvent Wash Draw Speed                      300 μL/min
Solvent Wash Dispense Speed                  3000 μL/min
Sample Wash Draw Speed                       300 μL/min
Sample Wash Dispense Speed                   3000 μL/min
Injection Draw Speed                         300 μL/min
Injection Dispense Speed                     6000 μL/min
Viscosity Delay                              2 sec
Sample Depth                                 Disabled
Injection Type                               Standard
L1 Airgap                                    0.2 μL
Solvent Wash Mode                            A, B

Sample Overlap
Mode                                         Sample overlap is not enabled


Front SS Inlet H2
Mode                                         Split
Heater                                       On    250 °C
Pressure                                     On    4.4452 psi
Total Flow                                   On    38.7 mL/min
Septum Purge Flow                            On    3 mL/min
Pre-Run Flow Test                            Off
Gas Saver                                    On    20 mL/min after 2 min
Split Ratio                                  50 :1
Split Flow                                   35 mL/min
Liner                                        A Liner has not been selected.

Column
Column #1
Flow
Setpoint                                     On
(Initial)                                    0.7 mL/min
Post Run                                     1 mL/min

Column Information                           Agilent 19091S-433UI: T330351H
Description                                  HP-5MS UI
Temperature Range                            -60 °C—325 °C (350 °C)
Dimensions                                   30 m x 250 μm x 0.25 μm (Uncalibrated)
Heater                                       Oven
Column lock                                  Locked
In                                           Front SS Inlet H2
Out                                          Front Detector FID
(Initial)                                    40 °C
Pressure                                     4.4452 psi
Flow                                         0.7 mL/min
Average Velocity                             21.646 cm/sec
Holdup Time                                  2.3099 min
Control Mode                                 Constant Flow

Column Outlet Pressure                       0 psi

Front Detector FID
Makeup                                       N2
Heater                                       On    300 °C
H2 Flow (Combined)                           On    30 mL/min
Air Flow                                     On    400 mL/min
Makeup Flow                                  On    20 mL/min
Carrier Gas Flow Correction                  Column + Fuel = Constant
Flame                                        On
Blank Evaluation Setpoints                   
Perform Blank Evaluation Test                Off

Detector Evaluation
Perform Detector Evaluation Test             Off

Signals
Signal #1:  Front Signal
Description                                  Front Signal
Details                                      Front Signal (FID)
Save                                         On
Data Rate                                    5 Hz
Dual Injection Assignment                    Front Sample

Signal #2: 
Description                                  None

Signal #3: 
Description                                  None

Signal #4: 
Description                                  None

Signal #5: 
Description                                  None

Signal #6: 
Description                                  None

Signal #7: 
Description                                  None

Signal #8: 
Description                                  None









=====================================================================
                              Column(s)
=====================================================================

Column Description :  HP-5MS UI
Inventory#         :  T330351H
Model#             :  19091S-433UI
Manufacturer       :  Agilent
Diameter           :   250.0 µm
Length             :   30.0 m
Film thickness     :    0.25 µm
Void time          :    2.310 min
Maximum Temperature:  325.0 °C
Comment            :  



